# What We Supply

### PVC-U / PVC-C Piping

Solvent-cemented systems for waterline and chemical-process routing, available across a wide size range with recognized international certifications.

### Polybutylene (PB) Piping

Flexible, lightweight piping joined by push-fit or fusion, built for chilled, hot, and cold water circuits.

### Stainless Steel Press Fittings

316L and 304 grade fittings sized 15mm–168.3mm, suited to chilled water, compressed air, and potable water runs on board vessels and inside hospitality and healthcare buildings.

### Thermoplastic PPR & PPR-CT

Welded polypropylene piping for hot and cold water distribution, chosen where corrosion simply isn't an option.

### Double Containment Pipe Systems

Layered PVC, CPVC, and stainless steel piping for transporting chemicals, compressed air, acid, and gas with a built-in secondary safety barrier.

### Stainless Steel / GI Drainage

Push-fit stainless drainage lines for waterline, wastewater, and seawater discharge — assembled without hot work.

### Carbon Steel Press Fittings

Press-jointed carbon steel components for heating circuits and cooling water networks in industrial settings.

### Copper & Bronze Press Fittings

Copper-based jointing for drinking water, gas, solar, and cooling applications where a clean, dependable seal matters.

### Acid Waste & PVDF Systems

Electrofusion and butt-fusion piping designed to hold up against aggressive chemicals — a fit for hospital labs and process plants alike.

### Neutralization Tanks

HDPE neutralization tanks ranging from 5 to 2,000 gallons, configurable with a range of lids, inlets, and outlets for hotel and hospital waste treatment.

### Valves, Strainers & Flow Control

A full valve line — ball, check, globe, butterfly, three-way, wafer, angle, diaphragm, gate — in metal and thermoplastic, built to DN and ASTM standards.